13.3 Configure the settings relating to H.264 recording [Alarm] (WV-SW559/WV-SP509)
Click the [Alarm] tab on the “Alarm” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the recording H.264 data on the SD memory card when an alarm is detected can be configured on this page. To operate recording, it is necessary to configure the settings relating to SD memory card and the video data. (→10.2 Configure the settings relating to the SD memory card [SD memory card] (WV-SW559/WV-SP509))
H.264 recording (SD memory card)
[Pre alarm]
Determine whether or not to perform the pre alarm recording. When “Use” is selected, approx. 1 MB image data is always saved during the pre alarm recording.
Use/ Not use
•
Default: Not use
[Post alarm (recording) duration]
Set the duration to save image data on the SD memory card after an alarm occurrence.
10s/ 20s/ 30s/ 40s/ 50s/ 60s/ 120s/ 180s/ 240s/ 300s
•
Default: 30s
* The actual recording time may sometimes be longer than the duration selected for this setting.
[Recording (memory) size per an alarm]
The capacity of the SD memory card used to record video data upon an alarm occurrence. The actual capacity may be different.
IMPORTANT
•
To record H.264 data, it is required to select “Use” for “SD memory card” on the [SD memory card] tab. In addition, it is required to select “H.264(1)” or “H.264(2)” for “Recording format”. (→10.2 Configure the settings relating to the SD memory card [SD memory card] (WV-SW559/WV-SP509))