16.2 Configure the settings relating to the FTP server [FTP]
Click the [FTP] tab on the “Server” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the FTP server used to transmit the alarm images can be configured on this page.
[FTP server address]
Enter the IP address or the host name of the FTP server.
•
Available number of characters: 1 - 128 characters
•
Available characters: Alphanumeric characters, the colon (:), the period (.), the underscore (_), and the hyphen (-).
IMPORTANT
•
When entering the host name for “FTP server address”, it is necessary to configure the DNS settings on the [Network] tab of the “Network” page. (→17.1 Configure the network settings [Network])
[User name]
Enter the user name (login name) to access the FTP server.
•
Available number of characters: 1 - 32 characters
•
Unavailable characters: " & : ; \
[Password]
Enter the password to access the FTP server.
•
Available number of characters: 0 - 32 characters
•
Unavailable characters: " &
[Control port]
Enter a control port number to be used for the FTP server.
•
Available port number: 1-65535
•
Default: 21
The following port numbers are unavailable since they are already in use.
20, 23, 25, 42, 53, 67, 68, 69, 80, 110, 123, 161, 162, 443, 995, 10669, 10670
[FTP mode]
Select “Passive” or “Active” for the FTP mode.
Normally, select “Passive”. When it is impossible to connect after select “Passive”, try to connect after selecting “Active”.
•
Default: Passive