1.3 Monitor cropping images
Full angle images and cropping images can be transmitted at the same time.
The cropping function must be configured in order to transmit cropping images. (→11.4 Configure the settings relating to the cropping function [JPEG/H.264])
H.264(2) or JPEG (VGA/QVGA/640x360/320x180) images can be set as cropping images.
By matching the settings of the “Compression” and “Stream” buttons on the “Live” page to the “Cropping” settings (“H.264”, “JPEG(VGA)/JPEG(640x360)”, or “JPEG(QVGA) /JPEG(320x180)”) configured on the [JPEG/H.264] tab, cropping images will be displayed on the [Cropping] display of the “Live” page and the main area.
Cropping
You can crop areas that you want to monitor.
By setting multiple cropping areas, up to 4 areas can be displayed in a sequence.
Sequence display using the cropping function
Note
•
The cropping function can be used only when “2 mega pixel [16:9]”, “1.3 mega pixel [16:9]”, or “1.3 mega pixel [4:3]” is selected for “Image capture mode”.