Section 12 Configure the multi-screen settings [Multi-screen]
The cameras from which images are to be displayed on a multi-screen can be registered on the “Multi-screen” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
[IP address]
Enter the IP address or the host name of the camera to be used for the multi-screen. 4 cameras can be registered as a group and up to 4 groups (16 cameras) can be registered.
When the HTTP port number for the camera of which images are to be displayed had been changed, enter as follows:
Example of entry:
–
Example when entering an IPv4 address: http://192.168.0.10:8080
–
Example when entering an IPv6 address: http://[2001:db8:0:0:0:0:0:1]:8080
•
Available number of characters: 1 - 128 characters
To access the cameras using the HTTPS protocol, enter as follows:
Example of entry: https://192.168.0.10/
IMPORTANT
•
When accessing the camera using the HTTPS protocol, install the security certificate of the camera to display images on the monitor. (→17.3.1 Install the security certificate)
Note
•
When using the host name, it is necessary to configure the DNS settings of the PC to be used for the multi-screen display. Refer to the network administrator for information on the DNS setting of PCs.
[Camera title]
Enter the title of the camera. The entered camera title will be displayed on a multi-screen.
•
Available number of characters: 0 - 20 characters
•
Unavailable characters: " &
Note
•
When selecting a 16 split-screen, some characters of the camera title to be displayed may not be displayed.
•
Even when “16:9” is selected for the aspect ratio, the multi-screen is displayed in 4:3.