13.7 Configuration of the settings relating to the mail notification [Notification]
Click the [Notification] tab on the “Alarm” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the alarm mail can be configured. It is necessary to configure the settings of the mail server to perform the mail notification. (→16.1 Configure the settings relating to the mail server [Mail])
Mail notification
[Mail server >>]
When “Mail server >>” is clicked, the [Mail] tab of the “Server” page will be displayed. (→16.1 Configure the settings relating to the mail server [Mail])
[Mail notification]
Select “On” or “Off” to determine whether or not to provide notification by e-mail according to the settings for the “Alarm” and “Diag.” checkboxes of “Destination of notification” below.
–
When an alarm is detected (“Alarm”)
:
–
When a notification of the remaining capacity of the SD memory card has been provided (“Diag.”)
–
When the SD memory card has become full (“Diag.”)
–
When the SD memory card cannot be recognized (“Diag.”)
•
Default: Off
[Alarm image attachment]
Select “On” or “Off” to determine whether or not to attach an image to the mail to be sent when an alarm is detected.
•
Default: Off
Note
•
The settings for “Image capture size” of the “Alarm image” section on the [Alarm] tab (→13.2 Configure the settings relating to the alarm image [Alarm]) will be applied to the size of the image to be attached.
•
When “3 mega pixel [4:3]” is selected for “Image capture mode”, images cannot be attached.
Destination of notification
[Address 1] - [Address 4]
Enter the destination mail address. Up to 4 destination addresses can be registered.
•
[Alarm] checkbox: When the checkbox is selected, the mail notification will be performed upon an alarm occurrence.
•
[Diag.] checkbox: When the checkbox is selected, the mail notification will be provided in the following cases.
–
When notification of the remaining capacity of the SD memory card has been provided
–
When the SD memory card has become full
–
When the SD memory card cannot be recognized
•
[Destination address]: Enter the destination address.
–
Available number of characters: 3 - 128 characters
–
Available characters: Alphanumeric characters, the at sign (@), the period (.), the underscore (_), and the hyphen (-).
To delete the registered address, click the [Delete] button respective to the desired address.
[Mail subject]
Enter the mail subject.
•
Available number of characters: 0 - 50 characters
[Mail body]
Enter the mail body.
•
Available number of characters: 0 - 200 characters
Note
•
Notification mail will be sent with the message “The capacity of the SD memory card is full.” when the SD memory card has become full, or “The SD memory card cannot be detected.” when mounting of the SD memory card failed.