11.11 Configure the VIQS area
The VIQS area is specified by following the steps below.
1.
Drag the mouse on the screen to specify the area (up to 2 areas).
→
The specified area is set to area “1(White)”, and the outline is displayed.
The areas are set in the area number order from number 1. The color next to the area number show the color of the corresponding outline.
Note
•
A selectable area is limited.
2.
Select [On]/[Off] to activate/deactivate a distributed image of [VIQS(H.264(1))] or [VIQS(H.264(2))].
3.
Click the [Set] button.
→
This unit is updated with the setting contents. Click the [Delete] button corresponding to the area to be deleted.
IMPORTANT
•
No setting contents are determined unless the [Set] button is clicked.
•
To check the window after VIQS setting, display an H.264 image on the “Live” page.