Viewer software
It is necessary to install the viewer software “Network Camera View 4S” to display images on a PC. This software can be installed directly from the camera or by selecting the [Install] button next to [Viewer Software] on the menu of the CD-ROM provided, and then following the on-screen instructions.
IMPORTANT
•
The default setting of “Automatic installation of viewer software” is “On”. Follow the instructions on Information Bar when the message is displayed on the information bar of the browser.
•
When the “Live” page is displayed for the first time, the install wizard of the ActiveX® control required to display images from the camera will be displayed. Follow the instructions of the wizard.
•
When the install wizard is displayed again even after completing the installation of the ActiveX, restart the PC.
•
The viewer software used on each PC should be licensed individually. The number of installations of the viewer software from the camera can be checked on the [Upgrade] tab of the “Maintenance” page (→19.2 Upgrade the firmware [Upgrade]). Refer to your dealer for the software licensing.