5.2 Transmit images at a designated interval or period (FTP periodic image transmission)
Images can be transmitted at a designated interval or period. To transmit images at a designated interval or period, it is necessary to configure the settings in advance.
The settings for the FTP server can be configured on the [FTP] tab of the “Server” page. (→16.2 Configure the settings relating to the FTP server [FTP])
It is possible to determine whether or not to use the FTP periodic image transmission function and to configure the settings relating to alarm images and the schedule on the “FTP img. trans.” tab of the “Network” page. (→17.6 Configure the settings relating to the FTP periodic image transmission [FTP img. trans.])
Note
•
Depending on the line speed or the traffic, images may not be transmitted at the designated interval.
•
When “On” is selected for both the alarm image transmission function and the FTP periodic image transmission function, the alarm image transmission function will be given priority over the FTP periodic image transmission function. Therefore, images may not be transmitted at the interval designated on the “FTP periodic image transmission” setting.