11.1 Configure the settings relating to the image capture mode [JPEG/H.264]
Click the [JPEG/H.264] tab on the “Image/Audio” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
[Image capture mode]
Select an image capture mode from the following.
2 mega pixel [16:9]/1.3 mega pixel [16:9]/1.3 mega pixel [4:3]/3 mega pixel [4:3]
•
Default: 2 mega pixel [16:9]
IMPORTANT
The positions of areas may move out of alignment when the “Image capture mode” setting is changed when the following area settings are configured. Therefore we recommend that you configure each area setting after configuring the “Image capture mode”.
–
mask area (→11.5.2 Set mask areas)
–
privacy zone (→11.9 Configure the settings relating to the privacy zone (Privacy zone setup menu))
–
VMD area (→13.6 Configure the VMD settings [VMD area])
–
VIQS area (→11.10 Configure the VIQS setting)
–
Cropping outlines (→1.3 Monitor cropping images)
Note
•
The other i-PRO series products do not support the aspect ratio of “16:9” unless otherwise stated. (As of December, 2011)
•
When “On” is selected for “VIQS” and the setting value for the aspect ratio is changed from “4:3” to “16:9”, make sure that the VIQS setting value does not exceed the maximum designated range.
•
When “3 mega pixel [4:3]” is selected, the following functions become unavailable.
–
“Image quality” for JPEG (the quality becomes “Quality1”)
–
H.264(2)
–
“Alarm image attachment” for mail notification
–
“Alarm image FTP transmission” for alarm
–
“FTP periodic image transmission” for periodic FTP transmission
–
“Cropping”
–
“Priority stream”