Section 7 Playback of images on the SD memory card (WV-SW559/WV-SP509)
When clicking a time and date listed on the log list window, the “Live” page will turn to the “Playback” page.
When images associated with the clicked time and date are on the SD memory card, the first image of them will be displayed.
IMPORTANT
•
This function is available only when “JPEG” is selected for “Recording format” of the SD memory card. When “H.264(1)” or “H.264(2)” is selected, the “Playback” page will not be displayed. However, images can be downloaded. Refer to 7.2 Download the images (When “H.264(1)” or “H.264(2)” is selected for “Recording format” of the SD memory card) for descriptions of how to operate.
•
Refresh interval of images may become slow during playback or download.
•
When many images are saved on the SD memory card, it may take time to display images on the “Playback” page.
•
Even when the size of the images saved on the SD memory card is “QVGA”, “1280x960”, or “2048x1536”, the images will be displayed in VGA size on the “Playback” page. When “16:9” is selected for the aspect ratio, images will be displayed in an image capture size of “640x360”, even “320x180”, “1280x720”, or “1920x1080” is selected. Therefore, images may look coarse on the “Playback” page.
•
When playing images by selecting an FTP error log on the log list, images may not be played in order of images recorded on the SD memory card if they have been recorded on the SD memory card with selected value for the “Transmission interval” setting on the [FTP img. trans.] tab is “1min” or less.
Number of images