13.1 Configure the settings relating to the alarm action [Alarm]
Click the [Alarm] tab on the “Alarm” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the alarm can be configured in this section. Refer to 13.2 Configure the settings relating to the alarm image [Alarm] and 13.4 Configure the settings relating to the alarm output terminal [Alarm] for further information about the settings relating to the alarm images and the alarm output terminal.
Alarm
[Terminal 1]
Determine how to use terminal 1.
•
Off: Not used.
•
Alarm input: Receives alarms.
•
Black & white input : Receives the black & white switchover input. (When the input is set to On, the black & white mode is activated.)
•
Default: Off
[Terminal 2]
Determine how to use terminal 2.
•
Off: Not used.
•
Alarm input : Receives alarms.
•
Alarm output: Alarm output will be carried out according to the settings for “Alarm output terminal setup” (→13.4 Configure the settings relating to the alarm output terminal [Alarm]).
•
Default: Off
[Terminal 3]
Determine how to use terminal 3.
•
Off: Not used.
•
Alarm input : Receives alarms.
•
AUX output: AUX output will be supplied. The [AUX] buttons will be displayed on the “Live” page.
•
Default: Off
Note
•
AUX is a camera terminal that allows users to operate (Open/Close) arbitrarily from the “Live” page. For example, an operator can remotely control lights in a place where the camera is installed by connecting the terminal to the light controller.
•
Refer to the installation guide for further information about input/output rating of each terminal.
•
While “Alarm input” is being selected, an alarm is detected when the terminal status is changed to “On”. (Default)
It is possible to configure the setting so that an alarm is detected when the terminal status is changed to “Off”. Refer to the [Readme] file on the provided CD-ROM for further information about the setting.
[VMD alarm]
When clicking “VMD >>”, the [VMD area] tab of the “Alarm” page will be displayed. (→13.6.1 Set the VMD areas [VMD area])
[Command alarm]
Select “On” or “Off” to determine whether or not to receive the command alarm.
The command alarm is the function that provides notification of a Panasonic protocol alarm from the other cameras. When “On” is selected, alarm actions will be performed between multiple cameras.
•
Default: Off
[Originating port number]
Select a port number to be used to receive the command alarm.
•
Available range: 1-65535
•
Default: 8181
The following port numbers are unavailable since they are already in use.
20, 21, 23, 25, 42, 53, 67, 68, 69, 80, 110, 123, 161, 162, 443, 554, 995, 10669, 10670, 59000-61000