11.4 Configure the settings relating to the cropping function [JPEG/H.264]
Click the [JPEG/H.264] tab on the “Image/Audio” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
[Cropping]
Select whether or not to transfer “JPEG” or “H.264(2)” as cropping images.
Off: cropping images are not transmitted.
H.264(2): H.264(2) is transmitted as cropping images.
JPEG(VGA)/JPEG(640x360): JPEG with a resolution of VGA or 640x360 is transmitted as cropping images.
JPEG(QVGA)/JPEG(320x180): JPEG with a resolution of QVGA or 320x180 is transmitted as cropping images.
•
Default: Off
Note
•
The cropping function can be used when “2 mega pixel [16:9]”, “1.3 mega pixel [16:9]”, or “1.3 mega pixel [4:3]” is selected for “Image capture mode”.
•
When changing the cropping position, use the cropping setup menu. (→11.4.1 Configure the settings related to cropping (Cropping setup menu))
•
Changing the cropping settings temporarily stops transmission.