5.3 Save images on the SD memory card when images fail to transmit using the FTP periodic image transmission function (WV-SW559/WV-SP509)
Images that have failed to transmit using the FTP periodic image transmission can be saved automatically on the SD memory card. It is possible to select a trigger to save images on the SD memory card on the [SD memory card] tab of the “Basic” page. (→10.2 Configure the settings relating to the SD memory card [SD memory card] (WV-SW559/WV-SP509))
To use the SD memory recording function featured in Panasonic network disk recorder, select “Off” for “FTP periodic image transmission” (→FTP periodic image transmission) and “FTP error” for “Save trigger” (→Common).
IMPORTANT
•
We make no guarantee for any damages of files on the SD memory card incurred by malfunction or error occurrence in files saved in the SD memory card regardless of what the cause may be.
Note
•
To refer to images of “FTP error”, “Save logs” needs to be set to “On” (→10.4 Configure the settings relating to the logs [Log] (WV-SW559/WV-SP509)).