17.3 Access the camera using the HTTPS protocol
1.
Start up the web browser.
2.
Enter the IP address of the camera in the address box of the browser.
•
Example of entry: https://192.168.0.10/
IMPORTANT
•
When the HTTPS port number is changed from “443”, enter “https://IP address of the camera + : (colon) + port number” in the address box of the browser.
(Example: https://192.168.0.11:61443)
•
When the camera is in a local network, configure the proxy server setting of the web browser (under [Internet Options...] under [Tools] of the menu bar) to bypass the proxy server for the local address.
3.
Press the [Enter] key on the keyboard.
→
The “Live” page will be displayed.
When the security alert window is displayed, install the security certificate. (→When using Internet Explorer 7, Internet Explorer 8, or Internet Explorer 9 - OS: Windows XP, Web browser: When using Internet Explorer 6)
When “On” is selected for “User auth.”, the authentication window will be displayed before displaying live images for the user name and password entries.
IMPORTANT
•
When the camera is accessed using the HTTPS protocol, the refresh interval and frame rate of images may be lower.