5.1 Transmit an alarm image at an alarm occurrence (Alarm image transmission)
An alarm image can be transmitted at an alarm occurrence to the FTP server. To transmit alarm images to an FTP server, it is necessary to configure the settings in advance.
The settings for the FTP server can be configured on the [FTP] tab of the “Server” page. (→16.2 Configure the settings relating to the FTP server [FTP])
The alarm image transmission function can be turned on/off in the “Alarm image” section of the [Alarm] tab of the “Alarm” page. (→13.2 Configure the settings relating to the alarm image [Alarm])
Note
•
Depending on the network traffic, the number of the transmitted images may not reach the set number of images to be transmitted.
•
Alarm images failed to be transmitted to the FTP server at an alarm occurrence will not be saved on the SD memory card. However, images that fail to be transmitted with the FTP periodic image transmission will be saved.