Section 6 Display the log list (WV-SW559/WV-SP509)
The setting items of the cameras will be displayed in list form.
•
Alarm log: Logs of the alarm occurrences such as time and date of the alarm occurrences and the alarm type will be displayed.
•
Manual/Schedule log: Logs filed when images have been recorded manually or during the period of the schedule on the SD memory card will be displayed.
•
FTP trans. error log: Logs filed when the FTP periodic image transmission function has failed will be displayed.
Each log list can be displayed only when “On” is selected for “Save logs” on the [Log] tab of the “Basic” page (→10.4 Configure the settings relating to the logs [Log] (WV-SW559/WV-SP509)) respectively.
1.
Display the “Live” page. (→1.1 Monitor images from a single camera)
2.
Click the [List] button.
→
The log list will be displayed in a newly opened window (log list window).
Number of the listed logs
IMPORTANT
•
Only a single user can operate the log list window. Other users cannot access the log list window.
Note
•
When “Not use” is selected for “SD memory card”, the “Manual/Schedule log” list and the “FTP trans. error log” list will not be displayed.
•
When “H.264(1)” or “H.264(2)” is selected for “Recording format” of the SD memory card, the “FTP trans. error log” list will not be displayed.
3.
Click the desired log type listed below “Log” to display the log list.
→ The log list of the selected log type will be displayed.
Note
•
When any images are saved on the SD memory card, the image can be displayed by clicking Time and Date when “JPEG” is selected for “Recording format” of the setup menu. (→10.2 Configure the settings relating to the SD memory card [SD memory card] (WV-SW559/WV-SP509))
About the log list window
Number of the listed logs
Total number of the logs of the selected log type and a number of the log being displayed on the top of the log list will be displayed.
Note
•
Enter the desired log number and press the [Enter] key on the keyboard. The log of the designated number will be displayed on the top of the log list.
[Top] button
Click this button to display the log listed at the top.
[Prev. page] button
Click this button to display the previous page of the log list.
Note
•
When the mouse button is held down while placing the mouse pointer on the [Prev. page] button, the displayed log number will be decreased. When the mouse button is released, the decrement of the log number will stop and the log number displayed at the moment when the mouse button is released will be the top of the currently displayed page.
[Next page] button
Click this button to display the next page of the log list.
Note
•
When the mouse button is held down while placing the mouse pointer on the [Next page] button, the displayed log number will be increased. When the mouse button is released, the increment of the log number will stop and the log number displayed at the moment when the mouse button is released will be the top of the currently displayed page.
[Last] button
Click this button to display the log listed at the bottom.
[Time & date]
Time and date when each log has been filed will be displayed.
Note
•
When “Off” is selected for “Time display format” (→10.1 Configure the basic settings [Basic]), time and date of alarm occurrence will be displayed in 24-hour format.
•
The recording timing of logs is as follows.
•
Alarm log: Alarm occurrence time and date will be filed as a log.
•
Manual/Schedule log: Time and date when recording of images onto the SD memory card started manually or during the period of the schedule will be filed as a log. When images are recorded sequentially, logs will be filed every one hour. However, depending on the photographic subject and the setting used, logs may be filed in periods of over on hour.
•
FTP trans. error log: Logs will be filed every one hour.
[Event]
The event type will be displayed. The event types will be displayed only when displaying the alarm log list.
•
TRM1: Alarm by alarm input to Terminal 1
•
TRM2: Alarm by alarm input to Terminal 2
•
TRM3: Alarm by alarm input to Terminal 3
•
VMD: Alarm by VMD alarm
•
COM: Alarm by command alarm
[SD memory card]
Available capacity and the original capacity of the SD memory card will be displayed.
The displayed descriptions are the same descriptions displayed as “Remaining capacity” on the [SD memory card] tab. (→SD memory card information)
[Delete] button
Click this button to delete the currently displayed log list.
When using the SD memory card, images associated with the log list will also be deleted.
IMPORTANT
•
When many images are saved on an SD memory card, complete deletion may take several hours. (For example, to delete 1 GB of JPEG images, approx. 1 hour may be needed.) In such a case, format the SD memory card. Be aware that formatting the SD memory card causes all the images to be deleted. (→SD memory card information)
•
In the process of the deletion, only logs will be saved, and it is impossible to save images newly.
•
Do not turn off the power of the camera until the deletion is complete. When the power of the camera is turned off in the process of the deletion, some images may remain on the SD memory card. In this case, click the [Delete] button on the same log list window used to delete the logs.
[Download] button
Click this button to download all logs of the selected log list as a file onto the PC.
[Close] button
Click this button to close the log list window.