11.10 Configure the VIQS setting
Click the [Setup>>] button of “VIQS” on the [Image quality] tab of the “Image/Audio” page. (→11.5 Configure the settings relating to image adjust, focus, back focus, extra zoom, privacy zone, VIQS, and lens distortion compensation [Image quality])
VIQS is an abbreviation of Variable Image Quality on Specified area and is a feature that enables you to change the images of a specified area.
It is possible to enhance the image quality of the specified range within a shooting area (image).
It is also possible to moderate the image data size by lowering the image quality of other areas.
The VIQS setting is available only for H.264 images.
Up to 2 VIQS areas can be set.
When checking the images after configuring the VIQS setting, display the H.264 images on the “Live” page.
[Delete]
Deletes the VIQS area. Click “Set” to delete the VIQS area.
[VIQS(H.264(1))]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(1)) images.
•
Default: Off
[VIQS(H.264(2))]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(2)) images.
•
Default: Off
IMPORTANT
•
After the VIQS setting is set to “On”, the VIQS area may move out of alignment when the JPEG/H.264 “Image capture mode” setting is changed. Make sure to check the VIQS setting after changing the “Image capture mode” setting.
Note
•
Refer to 11.11 Configure the VIQS area for setting procedure of the VIQS area.