11.6 Configure the focus setting (Focus setup menu) (WV-SW559/WV-SW558 only)
Click the [Setup>>] button of “Focus” on the [Image quality] tab of the “Image/Audio” page. (→11.5 Configure the settings relating to image adjust, focus, back focus, extra zoom, privacy zone, VIQS, and lens distortion compensation [Image quality])
Adjust the focus setting by moving the lens focus to the appropriate position.
Manual and auto adjustments are available.
The auto focus function also allows users to correct out of focus when changing between color and black & white images.
[Auto focus]
The auto focus function starts to automatically adjust focus based on a subject located in the center of the screen by clicking the [Execute] button.
[Focus]
The focus can be adjusted manually.
•
[Near] button: Click this button to adjust the focus to the “Near” side.
•
[Reset] button: Click this button to reset the focus to the default.
•
[Far] button: Click this button to adjust the focus to the “Far” side.
[Adjusting method]
Select the focus adjustment method upon switching between the color mode and the black & white mode.
•
Auto: Adjusts the focus function automatically and corrects out of focus when switching between color and black & white images.
•
Preset: Performs the preset movement to each specified focus position when switching between color and black & white images. The preset position is the focus position specified last time, which was automatically memorized for each of color images and black & white images.
•
Fix: Fixes the position after adjusting the focus either automatically or manually.
•
Default: Auto
[Close] button
Click this button to close the “Focus” setup menu.