19.4 Reset the settings/Reboot the camera [Default reset]
Click the [Default reset] tab of the “Maintenance” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings and the HTML data of the camera can be initialized and reboot of the camera can be performed on this page.
[Reset to the default (Except the network settings)]
Click the [Execute] button to reset the settings to the default. Note that the network settings will not be reset.
It is impossible to operate the camera for about 3 minutes after the initialization.
[Load the default HTML files (setup menu).]
Click the [Execute] button to reset the HTML files to the default.
It is impossible to operate the camera for about 3 minutes after the initialization.
[Reset to the default and load the default HTML files.]
Click the [Execute] button to reset the settings of the camera and the HTML files to the default. Note that the network settings will not be reset.
It is impossible to operate the camera for about 3 minutes after the initialization.
[Reboot]
Click the [Execute] button to reboot the camera. It is impossible to operate the camera for about 2 minutes after rebooting the camera.
Note
•
To initialize the network settings (→17.1 Configure the network settings [Network]), turn off the power of the camera, then turn on the power again while holding down the [INITIAL SET] button on the unit, and keep the [INITIAL SET] button held down for about 5 seconds. Wait about 3 minutes after releasing the button. The camera will start up and the settings including the network settings will be initialized. Do not turn off the power of the unit about 3 minutes after turning on the power.
:
•
The notification function allows users to provide the notification of the error to the specified destination mail address and an original alarm destination when an error such as no SD memory card insertion after the reboot or a locked SD memory card insertion occurs. (→13.7 Configuration of the settings relating to the mail notification [Notification], 13.8 Configure the settings relating to Panasonic alarm protocol [Notification])