Section 5 Transmit images onto an FTP server
Images can be transmitted to an FTP server. By configuring the following settings, transmission of images captured at an alarm occurrence or captured at a designated interval to an FTP server will become available.
IMPORTANT
•
When using this function, set the user name and the password to access the FTP server to restrict users who can log into the FTP server.
•
To transmit images to the FTP server, select “Not use” for “SD memory card”, or set “Save trigger” to “FTP error” on the [SD memory card] tab of the “Basic” page when “JPEG” is selected for [Recording format]. (→SD memory card)