10.4 Configure the settings relating to the logs [Log] (WV-SW559/WV-SP509)
Click the [Log] tab on the “Basic” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the log list can be configured in this section.
Alarm
Settings for the alarm log list can be performed.
[Save logs]
Select “On” or “Off” to determine whether to save the alarm logs.
•
On: Alarm logs will be saved.
•
Off: Alarm logs will not be saved.
•
Default: On
Note
•
When “Recording format” is set to “H.264(1)” or “H.264(2)”, “Save logs” is set to “On” or “Off” depending on the setting of “Save trigger”.
•
When “H.264(1)” or “H.264(2)” is selected for “Recording format” and when “Alarm input” is selected for “Save trigger”, only alarm logs will be saved.
[Name of the destination directory for downloaded images]
Enter the name of the destination directory to which images associated with the logs are to be downloaded. For example, enter “C:\alarm” to designate the folder “alarm” under drive C.
•
Available number of characters: 3 - 128 characters
•
Available characters: Alphanumeric characters, the slash (/), the backslash (\), the colon (:) and the underscore (_).
Manual/Schedule
Configure the settings relating to manual saving or schedule saving of the log list.
Select “On” or “Off” and designate the destination folder in the same manner as for “Alarm”.
Note
•
When “Recording format” is set to “H.264(1)” or “H.264(2)”, “Save logs” is set to “On” or “Off” depending on the setting of “Save trigger”.
•
Schedule saving is available only when “H.264(1)” or “H.264(2)” is selected for “Recording format”.
FTP error
Perform the settings for the FTP error log list.
Select “On” or “Off” and designate the destination folder in the same manner as for “Alarm”.
IMPORTANT
•
When “Name w/o time&date” is selected for “File name” on the [FTP img. trans.] tab on the “Network” page, FTP error log and associated images will not be saved. To save them, select “Name w/time&date”. (→17.6 Configure the settings relating to the FTP periodic image transmission [FTP img. trans.])
Note
•
When “H.264(1)” or “H.264(2)” is selected for “Recording format”, “FTP error” is unavailable.
•
When “3 mega pixel [4:3]” is selected for “Image capture mode”, “FTP error” is unavailable.