Section 18 Configure the settings relating to the schedules [Schedule]
On the “Schedule” page, it is possible to configure the settings relating to schedules as follows.
•
Alarm permission (Alarm input will be received only in the specified schedule.)
•
VMD permission (Video motion detection will be active only in the specified schedule.)
•
Access permission (Access to the camera will be allowed only in the specified schedule.)
•
H.264 recording (SD recording will be performed only in the specified schedule.)
The “Schedule” page has only the [Schedule] tab.
Up to 5 schedules can be set.
1.
Select an action to be assigned to the schedule from “Schedule mode”.
“Off” is selected at the default.
•
Off: No action will be taken for the respective schedule.
•
Alarm permission: Alarm input (terminal alarm) will be received during the period of the schedule.
•
VMD permission: The video motion detection (VMD) function will be active during the period of the schedule.
•
Access permission: Users whose access level is set to 2 and 3 on the “User auth.” tab (→15.1 Configure the settings relating to the user authentication [User auth.]) can access the camera only in the period of schedule.
•
H.264 recording : The SD recording will be performed at the designated time in the schedule.
Note
•
Select “On” for “User auth.” on the [User auth.] tab of “User mng.” page (→15.1 Configure the settings relating to the user authentication [User auth.]) and “Off” for “Host auth.” on the “Host auth.” page (→15.2 Configure the settings relating to the host authentication [Host auth.]) to validate “Access permission”.
•
When selecting “H.264 recording”, select “H.264(1)” or “H.264(2)” for “Recording format” on the [SD memory card] tab and select “Schedule” for “Save trigger”. (→10.2 Configure the settings relating to the SD memory card [SD memory card] (WV-SW559/WV-SP509))
2.
Select days of a week by checking the respective checkboxes.
3.
From the pull-down menu, select the start time and the end time of the schedule.
When not designating time, check the checkbox of “24h”.
4.
Click the [Set] button after completing the settings.
→
The result will be displayed at the bottom of the window.
Note
•
The schedules displayed at the bottom of the window can be identified by colors assigned to each schedule.