14.1 Configure the settings relating to the XML notification [XML notification]
Click the [XML notification] tab on the “Advanced func.” page.
The settings relating to the XML notification can be configured in this section.
The XML notification notifies the server of face detection information in XML format.
XML notification
[XML notification]
Select “On” or “Off” to determine whether or not to notify face detection information using XML.
•
Default: Off
[Notification data]
Select the type of data notification. One of the selections must be set.
•
Face data
Detection info.(Original)/Detection info.(Advanced)
Default: Detection info.(Original)
[Notification interval]
Select the notification interval.
•
Face data
1s/2s/3s/4s/5s/6s/10s/15s/20/s/30s/1min
Default: 1s
Note
•
When [Notification data] is set to “Detection info.(Original)”, the [Notification interval] can only be set to “1s” or “2s”.
Destination setting for XML notification
[Destination address]
Configure the IP address or the host name of the destination for XML notification.
•
Available number of characters: 1 - 128 characters
•
Available characters: Alphanumeric characters, the period (.), the underscore (_), and the hyphen (-).
[Destination port number]
Configure the port number settings for XML notification.
The following port numbers are unavailable since they are already in use.
20, 21, 23, 25, 42, 53, 67, 68, 69, 110, 123, 161, 162, 443, 995, 10669, 10670
[Destination path name]
Configure the settings for the destination directory to be used for the XML notification.
•
Available characters: Alphanumeric characters, the period (.), the underscore (_), the hyphen (-), the slash (/), and the colon (:).
[User name]
Enter a user name.
•
Available number of characters: 0 - 32 characters
•
Unavailable characters: " & : ; \
•
Default: None (blank)
[Password]
Enter a password.
•
Available number of characters: 0 - 32 characters
•
Unavailable characters: " &
•
Default: None (blank)