11.8 Adjust the angular field of view using the extra zoom function
Click the [Setup>>] button of “Extra zoom” on the [Image quality] tab of the “Image/Audio” page. (→11.5 Configure the settings relating to image adjust, focus, back focus, extra zoom, privacy zone, VIQS, and lens distortion compensation [Image quality])
It is possible to adjust the angular field of view using the extra zoom function.
•
: Click this button to adjust the zoom ratio to the “Wide” side.
•
: Click this button to set the zoom ratio to x1.0.
•
: Click this button to adjust the zoom ratio to the “Tele” side.
•
: Click this button to adjust the horizontal and vertical positions of the image after zooming.
IMPORTANT
•
The extra zoom function may not be activated on the appropriate position if the setting for the function is performed after the settings for the mask areas (→11.5.2 Set mask areas), privacy zone (→11.9 Configure the settings relating to the privacy zone (Privacy zone setup menu)), VMD area (→13.6 Configure the VMD settings [VMD area]), VIQS area (→11.10 Configure the VIQS setting). To prevent this, perform the setting for the extra zoom function before other settings.
•
When using the lens distortion compensation function, if the extra zoom function is used, the lens distortion compensation function is disabled.